Page1=LNB && Switch
Page2=Dish Setting
Page3=Filter
Page5=Statistics
Page10=Cable Setting
Page11=Filter
Page20=Terrestrial Setting
Page21=Filter
Ok=OK
Cancel=Cancel
Dialog1=Satellite Info/Channel Info
Dialog2=Transponder Info
Dialog3=PID Info
Dialog4=About VisionData
String1=This transponder already exist.
String2=Can not reach this satellite from your location!
String3=Cann't input more than four chars.
String4=Input Data PID between Hex: 0015-1FFE.
String5=Input Data PID between Dec: 21-8190.
String6=This PID already exist.
String7=Are you sure to remove the current PID?
String8=Please successfully lock current transponder at first.
String9=The filter don't start, please lock again.
String10=Can't unload this PID, please try it again.
String11=This value must be less than 45000.
String12=Error! PID Data can`t be empty!!!
String13=Input Data PID between 21 and 8190 (Hex: 0015-1FFE)!
String14=Degree value must be 0--3600.
String15=Frequency data is invalid, it must be 950-14000.
String16=Symbol rate data is invalid, it must be 900-45000.
String17=Polarity is invalid.
String18=Can't initialize hardware infomation, reboot Windows?
String19=This satellite already exists.
String20=Are you sure to remove the current satellite?
String21=Can't stop filter, so we can't remove current transponder.
String22=The current transponder already changed. The locked transponder is not the current transponder, please lock the current transponder at first.
String23=Log file's size is bigger than 50M bytes. Do you want to clear it? If not, It cann't save any log message.
String24=Locking, Please wait......
String25=The application will exit, save current changed settings and data?
String26=The application will restore settings and data, are you sure?
String27=Are you sure to remove the current transponder?
String28=Scanning, Please wait......
String29=Are you sure to remove all transponders?
String30=This channel already exists.
String31=Are you sure to remove the current channel?
String32=Please successfully lock current channel at first.
String33=The current channel already changed. The locked channel is not the current channel, please lock the current channel at first.
String34=Fail to load this PID
String35=Fail to unload this PID
String36=Hide
String37=Show
String38=About
String39=Exit
String40=Satellite name can`t be empty!
String41=Satellite degree value can`t be empty! 
String42=Fail to read the hardware's MAC address. Please reboot Windows and try again!
String43=MAC address initialized, reboot Windows for the MAC address to take effect?
1001=Satellite list/Channel list
1003=Satellite/Channel
1004=New
1005=Edit
1006=Remove
1008=Help
1009=Apply
1011=Language
1013=Strength
1014=Quality
1017=Dish Type
1018=Fixed
1019=DiSEqC 1.2 (motor)
1020=USALS (motor)
1021=LNB Power
1022=22KHz Tone
1030=Vertical
1031=Horizontal
1036=Add
1037=Remove
1038=Set East Limit
1039=Set West Limit
1040=Cancel Limit
1041=Goto Zero
1042=Goto Satellite
1043=Decimal
1044=Hexadecimal
1045=Set Multicast PIDs automatically
1046=Use the MAC address of the hardware 
1047=Caculate MAC address from IP address of Dial-up connection
1048=Caculate MAC address from IP address of network interface card
1049=Caculate MAC address from the following IP address
1054=IP-Data Version 1.8.0.1
1055=Copyright (C) 2004-2006
1056=OK
1057=Satellite
1058=Dish options
1059=Dish Type
1060=Satellite
1061=Degree
1065=Transponder options
1066=Transponder
1067=Frequency
1068=Symbol Rate
1072=Polarization
1073=Motor Settings
1074=Longitude
1075=Latitude
1076=Degrees
1077=Elevation
1079=Drive East
1080=Drive West
1081=Lock Test
1082=Scan....
1083=Unicast(internet) Filter setting
1084=IP to MAC prefix
1087=Default PIDs
1088=Unicast PID
1089=Broadcast PID
1090=Multicast PID
1094=Proxy IP address
1095=Proxy IP address
1096=Port
1098=Load
1099=Unload
1100=LNB Setting
1101=LNB
1102=LNB Freq.1
1103=LNB Freq.2
1105=DiSEqC
1106=Tone/Data
1111=Name
1112=Degree
1113=New
1115=Symbol Rate
1116=Frequency
1118=Vertical
1119=Horizontal
1129=Hexadecimal(0015-1FFE)
1130=Decimalization(21-8190)
1131=PID Data:
1132=Remove
1134=Frequency:
1137=KHz(40000 ~ 870000 KHz)
1141=Symbol Rate:
1143=Ksps(0 ~ 7000 Ksps)
1144=QAMSize:
1150=Channel Info
1151=Lock Test
1157=Switch Setting
1159=PID Type:
1162=MHz
1163=Ksps
1164=MHz
1165=Ksps
1166=Restore
1167=Motor Position
1168=Position:
1170=Goto
1171=Set
1173=Data statistic
1176=Bytes
1177=Receive
1178=Error
1179=Total
1180=Packets
1181=Receive
1182=Error
1183=Total
1184=Speed
1193=Mbytes
1194=Mbytes
1195=Mbytes
1196=KPackets
1197=KPackets
1198=KPackets
1199=Kbps
1200=Lock Test
1201=Full Scan
1202=Frequency
1204=BandWidth
1206=Step
1208=Channel Info
1209=KHz(51000 ~ 860000 KHz)
1210=MHz
1211=MHz(1 ~ 8 MHz)
1212=MAC Address
162=Change MAC Address
1214=Change
1221=Save
1222=Set MAC Address by Registry
1235=MAC Address Setting (Hexadecimal)
1236=Current MAC Address
1237=New MAC Address
